{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":21,"n_cols":12,"rows_kept":21,"cut":false,"hidden":false,"merged":[]}
["Address","RegisterType","OperationType","DataType","ScpiCommand","DeviceTarget","TriggerValue","DataAddress","DataAddressType","ScaleFactor","ResponseAddress","Description"]
[100,"Holding","Write","Int16","*RST","APS7100",1,null,null,1,101,"复位设备"]
[100,"Holding","Write","Int16","*CLS","APS7100",2,null,null,1,101,"清空设备"]
[100,"Holding","Write","Int16","SYST:REM","APS7100",3,null,null,1,101,"远程模式"]
[100,"Holding","Write","Int16","SYST:LOC","APS7100",4,null,null,1,101,"本地模式"]
[100,"Holding","Write","Int16","OUTP ON","APS7100",5,null,null,1,101,"输出打开"]
[100,"Holding","Write","Int16","OUTP OFF","APS7100",6,null,null,1,101,"输出关闭"]
[100,"Holding","Write","Int16","SOUR:VOLT {0}","APS7100",7,110,"Float",1,101,"设定电压"]
[100,"Holding","Write","Int16","SOUR:FREQ {0}","APS7100",8,112,"Float",1,101,"设定频率"]
[100,"Holding","Write","Int16","SOUR:CURR {0}","APS7100",9,114,"Float",1,101,"设定限制电流"]
[200,"Holding","Read","Float","MEAS:CURR?","APS7100",null,null,null,1,null,"读取当前测试电流"]
[300,"Holding","Write","Int16","*RST","PSW250",1,null,null,1,301,"复位设备"]
[300,"Holding","Write","Int16","*CLS","PSW250",2,null,null,1,301,"清空设备"]
[300,"Holding","Write","Int16","SYST:REM","PSW250",3,null,null,1,301,"远程模式"]
[300,"Holding","Write","Int16","SYST:LOC","PSW250",4,null,null,1,301,"本地模式"]
[300,"Holding","Write","Int16","OUTP ON","PSW250",5,null,null,1,301,"输出打开"]
[300,"Holding","Write","Int16","OUTP OFF","PSW250",6,null,null,1,301,"输出关闭"]
[300,"Holding","Write","Int16","FUNC:MODE CURR","PSW250",7,null,null,1,301,"设定电流模式"]
[300,"Holding","Write","Int16","SOUR:CURR {0}","PSW250",8,310,"Float",1,301,"设定电流值"]
[300,"Holding","Write","Int16","SOUR:VOLT:PROT {0}","PSW250",9,312,"Float",1,301,"设定过压保护值"]
[400,"Holding","Read","Float","MEAS:VOLT?","PSW250",null,null,null,1,null,"读取当前测试电压"]